{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":285,"n_cols":12,"rows_kept":285,"merged":[[0,0,0,11],[1,0,1,3],[1,4,1,11],[281,0,281,11],[282,0,282,11],[283,0,283,11],[284,0,284,11]]}
["2018年工器具选型清单"]
["需求描述",{"$nulls":3},"供应商提报描述"]
["序号","物资名称","物资参数","单位","品牌型号1","参数1","报价1","品牌型号2","参数2","报价2","......","备注"]
[1,"1/4转1/4六角接杆变方头转换器","六角头为6.3mm通用接口，方头带弹性钢珠","个/只/台"]
[2,"1/4转3/8六角接杆变方头转换器","六角头为6.3mm通用接口，方头带弹性钢珠","个/只/台"]
[3,"1/4转1/2六角接杆变方头转换器","六角头为6.3mm通用接口，方头带弹性钢珠","个/只/台"]
[4,"装卸运送推车","采用不锈钢材质，拉杆，带刹车，一侧带小钭，小钭宽度与箱体宽度一致600MM，橡胶轮，承重力500Kg，规格（箱体净高）：长*宽*高：800*600*800MM，需加装带锁装置，需运营方样品确认。","个/只/台"]
[5,"水平尺","600mm","个/只/台"]
[6,"数显游标卡尺","量程0-300mm，精度0.03mm","个/只/台"]
[7,"红外线测温仪","测量范围-32℃～400℃;交叉式双激光照准;测量物距比121","个/只/台"]
[8,"温湿度计","煤油型棒式","个/只/台"]
[9,"可调直流稳压电源","36V/3A ","台"]
[10,"LED带灯反光镜","带伸缩杆，镜头360度旋转","个/只/台"]
[11,"数字兆欧表","测试直流电压5000V","个/只/台"]
[12,"钢卷尺","7.5m","个/只/台"]
[13,"氩气减压阀总成","YQAR-731L;输入压力15MPA;输出压力0.15MPA;流量0-15L/MIN","个/只/台"]
[14,"掉线锤","锤头不锈钢，线长6m，0.5kg","个/只/台"]
[15,"数显水平尺","600mm","个/只/台"]
[16,"T型内六角扳手","T型，公制，8mm","个/只/台"]
[17,"水平尺","HG200-1B","个/只/台"]
[18,"中功率计","频率范围：DC~4GHZ，功率测试范围：1MW~25W，1W~100W功率探头：≤±4％，衰减精度：≤±0.5DB，驻波系数：≤1.3，连接形式：N,LL6-50Ω电源：DC9V，100W衰减器","个/只/台"]
[19,"光照度计","测量范围自0.01Lux至999900 Lux、0.001fc至99990 fc，计5档自动换档","个/只/台"]
[20,"氧气表","YQY-08，氧气减压器","个/只/台"]
[21,"乙炔表","YQE-03，乙炔减压器","个/只/台"]
[22,"第四种检查器","JLJ-4C，测量范围：圆周磨耗为0-9mm，轮缘高度为22-37mm","个/只/台"]
[23,"车钩高度尺","GF206-T，铁路专用，测量范围 650-950mm ","把"]
[24,"车门夹紧力测量仪","PINCH FORCE METERSYSTEM BIA (2-10)专用","个/只/台"]
[25,"频率计","10Hz-2.4G频率测量范围，8位LED显示","个/只/台"]
[26,"手持式2M测试仪","规格尺寸：SMARTCLASS E1，技术参数：SMARTCLASS E1","个/只/台"]
[27,"逻辑分析仪","输入通道：32个数据采样通道，2个外部时钟通道；门限电压：6个独立可调的门限电压；调节范围：-6V～+6V，分辨率：0.1V","台"]
[28,"相序检测器","电压范围：40-690V；频率范围15-400Hz","个/只/台"]
[29,"数显游标卡尺","量程0-200mm，精度0.02mm","个/只/台"]
[30,"微量水分检测仪","集森：JLD242","个/只/台"]
[31,"指针式测力计","最大负荷10N、分度值0.05N、最小测量值1N、精度±1%、工作温度±10℃","个/只/台"]
[32,"低电阻测量仪","量程:0.01μΩ-200Ω","个/只/台"]
[33,"涂层测厚仪","具有两种测量方式：连续测量方式(CONTINUE)和单次测量方式(SINGLE)；具有两种工作方式：直接方式(DIRECT)和成组方式(Appl)；设有五个统计量：平均值(MEAN)、最大值(MAX)、最小值(MIN)、测试次数(NO.)、标准偏差(S.DEV)；","个/只/台"]
[34,"蓄电池智能放电测试仪","放电电流：0-30A连续可调，分辨率0.1A，精度1A;放电总电压：300-600V，分辨率10mV，精度0.1V；放电单体电压：0-16V,分辨率1mV，精度10mV","个/只/台"]
[35,"蓄电池智能放电测试仪","通信48V蓄电池组维护,充放电功率6KW,放电电压范围DC 18-60V,充电电流100A","个/只/台"]
[36,"接触网导线磨耗测量仪","测量高度:1m～6.5m，适用范围:CT85、CT100、CT110、CT120、CT150、CT250，测量精度:0.01mm","个/只/台"]
[37,"指针式测力计","承受拉力:不得低于5T，刻度显示:1刻度1KN（100KG）","个/只/台"]
[38,"接地电阻测试仪","0-1-10-100，13.01级","个/只/台"]
[39,"数字兆欧表","测量测试电压:5kVDC，测量范围:10TΩ","个/只/台"]
[40,"红外热像仪","温度测量范围:（-10℃以下未经校准）-20℃～+600℃(-4℉～+1112℉)，准确度:±2℃或者2%、取大值","个/只/台"]
[41,"数字压力表","范围从 0~70 mbar至700 bar,16种压力单位","个/只/台"]
[42,"氧化锌避雷器带电测试仪","测量范围:电流:0-20mA ,电压：0～220V ,分辨率:0.001,测量精度   基波：±(5%读数+5字), 谐波：±(10%读数+10字) ,传输距离   500米（可视距离）","个/只/台"]
[43,"任意波形发生器","直流电流输出：0～24mA 精度：量程的0.05%;直流电压输出：0～10V 精度：量程的0.1%;配电电压输出：直流24V;供电电压：交流220V","个/只/台"]
[44,"高压开关特性测试仪","1．时间测量\n同时可测量断口数：≤12个\n测定过程整定时间：0～6秒\n分辨率：0.1ms\n2．开关开距、开关超行程、弹跳幅度测量\n量程：<1000mm\n分辨率：1mm\n3．测量误差\n时间测量误差：±1%\n行程测量误差：±1%.\n4．速度测量范围：0～20m/s","个/只/台"]
[45,"辙叉磨耗测量器","适用于P60钢轨","个"]
[46,"数字万用表","FLUKE;F179","个/只/台"]
[47,"温湿度计","温度：-20℃ ~ 60℃ (-4℉ ~ 140℉) \n湿度：10%RH ~ 95%RH，分辨率0.1℃/0.1℉/0.1%RH，准确度温度：±0.5℃、±0.9℉ \n湿度：±3%RH(25℃时30~95%RH);±5%RH(25℃时10~30%RH)","套"]
[48,"蓄电池内阻测试仪","测量范围：内阻0.000mQ-99.999mQ，电压0-25V；最小测量分辨率：内阻0.001mQ，电压1mV；测量精度：内阻±0.5%rdg ±6dgt，电压±0.2%rdg ±6dgt","个/只/台"]
[49,"手持式数字示波器","通道数2，60 MHz、100 MHz或200 MHz带宽，实时采样率高达2.5 GS/s，400 ps分辨率","个/只/台"]
[50,"红外线热成像仪","探测器分辨率160*120（19200像素），最小焦距15cm（6in）","个/只/台"]
[51,"网络测试仪","工作温度32℉到101℉，振动：随机、2g、5Hz-500Hz","个/只/台"]
[52,"真有效值数字钳形表","交流电流：量程10-1000A，分辨率0.01-1A；交流电压：量程400V/750V，分辨率0.1V/1V；直流电压：量程400V 1000V分辨率0.1V/1V；电阻：量程400Ω 4000Ω，分辨率0.1Ω/1Ω","个/只/台"]
[53,"接地电阻测试仪","接地电阻测量范围：0.1Ω~1000Ω；误差：≤±3%；最小分辨率为：0.01Ω；漏电流测量范围：0.10-3.0A；存储容量：200组数据\n；工作温度：0ºC ~ + 50°C","个/只/台"]
[54,"电池盒/电流和电压校准器","Timeelectronics;1044voltograndcurrentcalibrator","套"]
[55,"数字交直流钳形表","交流电流 200mA/2/20A，±1%rdg±2dgt(200mA)(50/60Hz)，±1.5%rdg±4dgt(200mA)(40-2kHz)，±1%rdg±2dgt(2A)(50/60Hz)，±2.5%rdg±5dgt(2A/20A)(40Hz-2kHz)；直流电流2/20A，±1%rdg±2dgt（2A），±1.5%rdg±4dgt（20A）","套"]
[56,"数显式测力计","500N公制50kg，精度±0.5%","个/只/台"]
[57,"主控量规","VOITH，230.011605","个/只/台"]
[58,"指针式测力计","单针式，测量范围0-5N，精度等级2，分度值0.5，横向测力计","个/只/台"]
[59,"套筒","12.5MM系列，6角标准型，14MM","个/只/台"]
[60,"套筒","12.5MM系列，6角标准型，17MM","个/只/台"]
[61,"套筒","12.5MM系列，6角标准型，19MM","个/只/台"]
[62,"套筒","12.5MM系列，6角标准型，22MM","个/只/台"]
[63,"套筒","12.5MM系列，6角加长型，22MM","个/只/台"]
[64,"套筒","12.5MM系列，6角加长型，24MM","个/只/台"]
[65,"光纤电缆剥线钳","5\"，剥线范围:0.2-0.8mm²","把"]
[66,"高压风管","内径Φ9MM，耐压:10kg","米(m)"]
[67,"电焊锤","350MM，800g","个/只/台"]
[68,"信号旗","含红、黄、绿各一面","套"]
[69,"铜管切管器","切割范围：6-64MM","个/只/台"]
[70,"圆吊带","1T，2m","个/只/台"]
[71,"圆吊带","4T，8m","个/只/台"]
[72,"司机工作箱包","95*290*400MM;包内框架材质201#不锈钢，厚度1.2MM","个/只/台"]
[73,"退播针工具","使用于哈丁插头的退播针用，0.5-1.5mm，长度约10cm","个/只/台"]
[74,"手动抽油泵","油罐口螺纹M64*4和G2，用于容积200L油罐","个/只/台"]
[75,"活动扳手","15\"，沾塑","个/只/台"]
[76,"两用扳手","36mm，公制","个/只/台"]
[77,"两用扳手","30mm","个/只/台"]
[78,"梅花扳手","东工;GJ-62","个/只/台"]
[79,"扭矩扳手开口板子头","10.19，A=19MM E=9MM B=41.5MM L=20MM","个/只/台"]
[80,"扭矩扳手开口板子头","10.13，A=13MM E=7MM B=29MM L=17.5MM ","个/只/台"]
[81,"扭矩扳手开口板子头","10.15，A=15MM E=9MM B=33MM L=20MM","个/只/台"]
[82,"扭矩扳手开口板子头","10.16，A=16MM E=9MM B=35.5MM L=20MM","个/只/台"]
[83,"扭矩扳手开口板子头","10.17，A=17MM E=9MM B=37.5MM L=20MM","个/只/台"]
[84,"扭矩扳手开口板子头","10.18，A=18MM E=9MM B=39MM L=20MM","个/只/台"]
[85,"Y型六角套筒扳手","规格尺寸：8*9*10MM，尺寸32*22*26","个/只/台"]
[86,"发黑内六角扳手","12MM，L型，黑色","个/只/台"]
[87,"发黑内六角扳手","14MM，L型，黑色","个/只/台"]
[88,"发黑内六角扳手","16MM，L型，黑色","个/只/台"]
[89,"水泵钳","16\"，适用管子直径：10-92MM","把"]
[90,"皮带管钳","11\"","把"]
[91,"风道扎带夹钳","公称通径 4.8mm（mm），紧固直径 10-300（mm） ，手动紧带机 ","把"]
[92,"电动螺丝批","最大扭矩:25N.M，GSR 14.4-2","套"]
[93,"油灰刀","3寸，不锈钢，塑柄","把"]
[94,"木柄钳工锤","锤头材质:高碳钢，长度:360mm，重量:1000g","把"]
[95,"橡胶锤","24oz","把"]
[96,"防震橡胶锤","53oz","把"]
[97,"两爪真空吸盘","100KG","个/只/台"]
[98,"六角撬棍","φ28*1500MM，鸭嘴型","根"]
[99,"铁路开口撬棍","行业通用类;，φ25*1500MM，材质:实心钢","根"]
[100,"配票箱/镀锌","500mm*380mm*690mm，拉杆箱，不锈钢材质，带刹车","个/只/台"]
[101,"油盒","600*400*100MM，不锈钢，在长度方向两侧安装把手","个/只/台"]
[102,"零件盒","300*450*177MM，塑料材质","个/只/台"]
[103,"工具提包","450*230*300mm，不含工具","个/只/台"]
[104,"手摇道岔工具包","440*300*300，不含工具","个/只/台"]
[105,"工具包","200*300*100MM","个"]
[106,"道岔备品箱","80*40*30CM;含盖和锁","个/只/台"]
[107,"手提钢制工具箱","20\"，510*220*240，不含工具","个/只/台"]
[108,"黄油嘴","直头;6MM","个/只/台"]
[109,"黄油嘴","弯头;8MM，90°","个/只/台"]
[110,"手动黄油枪软管","18\"，长度450MM，高强度耐压尼龙套，可方便插入工作区域","个/只/台"]
[111,"热风枪","大有;7701;2000W","个/只/台"]
[112,"钻头组套","配合喜利得TE-50电锤钻使用，TE-Y\"速钻\"五坑两刃钻头组套（直径12mm，总长350mm，工作长度200mm，1根；直径14mm，总长350mm，工作长度200mm，1根；直径16mm，总长350mm，工作长度200mm，1根；直径22mm，总长320mm，工作长度200mm，1根；直径24mm，总长320mm，工作长度200mm，1根）","套"]
[113,"梯车","工作台高4米","个/只/台"]
[114,"门式脚手架","材料工艺：Q235，管壁厚:2.0MM，技术参数：工作高度：2M，承重：500KG，配套两块踏板，四个套筒","个/只/台"]
[115,"吊装带","5T，2m","个/只/台"]
[116,"吊装带","5T，1.5m","个/只/台"]
[117,"退针器","用于AMP接头","套"]
[118,"线坠","500g ","个/只/台"]
[119,"吹尘球","材质：PVC，长11.7cm，球径5.5cm","个/只/台"]
[120,"铁字模","阿拉伯数字，字高35mm","套"]
[121,"铁字模","特殊符号，字高35mm","套"]
[122,"铁字模","英文字母，字高35mm","套"]
[123,"剥线钳","6\"，剥线范围：美制电线标准 截面积 20-30AWG 0.52-0.052","把"]
[124,"十字绝缘螺丝批","#3*150mm","把"]
[125,"直刃式电缆割刀","VDE绝缘、耐压1000V，直刃式","个/只/台"]
[126,"扭矩扳手开口板子头","10.14，A=14MM E=7MM B=31.5MM L=20MM","个/只/台"]
[127,"除湿机","日除湿量：＞21L/D，适用面积：＞100㎡，额定功率：1450W，电源电压：220V","个/只/台"]
[128,"气风枪喷嘴","BACO;958 105 15A;直径3MM，长260MM","个/只/台"]
[129,"气风枪喷嘴","BACO;958 470 76;直径3MM，长800MM","个/只/台"]
[130,"气风枪喷嘴","BACO;958 105 107;直径3MM，长415MM","个/只/台"]
[131,"尼龙气枪","BACO;958 470 140;工作气压2-6BAR，最大工作气压10BAR","把"]
[132,"闸瓦间隙调整扳手","闸瓦间隙调整扳手","个/只/台"]
[133,"量杯(含搅拌棒)","500ml","个/只/台"]
[134,"手摇巡检工作灯","具有手摇充电应急功能，满足灯具人工快速充电的需求。手摇100/min，一分钟，使用30min。具有给手机充电的功能，满足手机应急充电的需求。额定电压：3.7V，强光：8h，工作光：35h，泛光：42h","个/只/台"]
[135,"接触线煨弯器","张垣;适用80～120mm2导线、地铁接触线","个/只/台"]
[136,"轻便式强光灯","连续放电时间h≥10，充电时间h=6","个/只/台"]
[137,"便携式高速电锯","切断能力:地下电缆120mm，管材120mm，使用电压:AC220V，功率:650W（含锯条）","个/只/台"]
[138,"接触线扭面器","NM-V，适用各种线型","个/只/台"]
[139,"接触线校直器","5轮，适用于120mm2，150mm2接触线，适用张力范围：10KN-20KN","个/只/台"]
[140,"充电手电钻套装","最大夹持13MM，18V，135N.M，2电1充","个/只/台"]
[141,"两用扳手","开口24MM，全抛光","个/只/台"]
[142,"工具组套","25件工具组套","套"]
[143,"芯线压线钳","VS.JJ1;信号电缆接续使用","把"]
[144,"圆吊带","3T，5m","个/只/台"]
[145,"圆吊带","3T，8m","个/只/台"]
[146,"圆吊带","5T，8m","个/只/台"]
[147,"电动喷雾器","蓝艺背负式电动喷雾器；16L；","个"]
[148,"焊炬通针","通用类;不锈钢材质，10支/套","个/只/台"]
[149,"双向棘开两用快扳","公制，16mm，精抛光","把"]
[150,"双向棘开两用快扳","公制，19mm，精抛光","把"]
[151,"工具组套","A54:N70,拓为;780122","套"]
[152,"工具组套","28件基本维修组套","套"]
[153,"门式脚手架","材料工艺：Q235，管壁厚:2.0MM，技术参数：工作高度: 1M，承重: 500KG，配套两块踏板，四个套筒","个/只/台"]
[154,"单开口扳手","46mm","套"]
[155,"6角旋具套筒","17mm","套"]
[156,"链条扳手","24\"","把"]
[157,"可调恒温热熔胶枪","NL-308","个"]
[158,"自切底锚栓安装工具","22*80-M16","个/只/台"]
[159,"扩孔工具","22-M16;2084510","个/只/台"]
[160,"限位钻头","22*125-M16","个/只/台"]
[161,"磁性捡拾器","头径8MM，长度400MM，捡拾重量0.5KG","个/只/台"]
[162,"手摇注油器","博洛克;PH-45611;手摇加注器，齿轮油加注器，重量4kg","个/只/台"]
[163,"套筒组套","F型套筒扳手，32件套，含7-32mm套筒26件、长、段接杆各1件、弯柄1件、棘轮扳手1件、快速盘1件、快速摇柄1件","套"]
[164,"双开口扳手组套","9件套，(8*10MM，9*11MM，10*12MM，12*14MM，14*17MM，17*19MM，19*22MM，24*27MM，30*32MM)，全抛光","套"]
[165,"精密雕刻刀","不锈钢，全长150mm，刀刃角度是30°,配30片KB-3刀片","只"]
[166,"脚踏型黄油机","管长4米，容量6L，最大输出压力20Mpa","个/只/台"]
[167,"套筒","19MM系列，12角套筒，34mm","个/只/台"]
[168,"套筒","19MM系列，12角套筒，36mm","个/只/台"]
[169,"套筒","19MM系列，12角套筒，38mm","个/只/台"]
[170,"充电式可调恒温电烙铁","华雨多功能便携式可充电电烙铁可调温恒温可移动焊台户","套"]
[171,"高压水枪","电压220v；功率1800W；+15米水管+高压长短两用枪头","个/只/台"]
[172,"十字螺丝批","PH2*100mm;捷德纸币机大修需使用工器具，HARDEN，55376 经查为#6*100mm","个/只/台"]
[173,"尖嘴钳","6\";捷德纸币机大修需使用工器具，PLIERS，SHP-L160D","个/只/台"]
[174,"防滑棘轮扳手(三个转接头）","RT1/4;捷德纸币机大修需使用工器具","个/只/台"]
[175,"两用快扳","7mm","个/只/台"]
[176,"两用快扳","5.5mm","个/只/台"]
[177,"钩N型弹簧钩","205mm，捷德纸币机大修需使用工器具","个/只/台"]
[178,"平头T柄内六角","捷德纸币机大修需使用工器具","个/只/台"]
[179,"人字伸缩梯","铝合金，3.8米，工程伸缩梯，德标人字梯","把"]
[180,"短柄棘轮螺丝批组套","25件套，世达;09342;捷德纸币机大修需使用工器具","套"]
[181,"恒温PPR管热熔器","技术参数：20-63MM：能热熔管径20MM 25MM 32MM 40MM 50MM 63MM","个/只/台"]
[182,"PVC管子割刀","适用于50-120mm的PPR/PE/PVC塑料水管","把"]
[183,"电磨机","220V/50HZ，最大磨轮直径25mm，最大夹头直径8mm（标配6mm），空载转速33000R/MIN，额定输入功率500W","个/只/台"]
[184,"电焊焊钳","纯铜电焊钳，500型，长度270mm","个/只/台"]
[185,"电焊地线夹子","500A，铜质","个/只/台"]
[186,"钢板起重钳","起重载荷2T","个/只/台"]
[187,"铸铁方箱","规格300*300*300，材质为HT200-300","个/只/台"]
[188,"划线平台底座","规格1000*1000mm，可调支架底座，与划线平台配套使用","个/只/台"]
[189,"钻头组套","直柄麻花钻，直径Ф4-Ф12","套"]
[190,"丝锥组套","21件套，M3-M12套装，头锥/二锥/尾锥:M3*0.5、M4*0.7、M5*0.8、M6*1.0、M8*1.25、M10*1.5、M12*1.75","个/只/台"]
[191,"板牙组套","M4-M12套装，M3*0.5、M4*0.7、M5*0.8、M6*1.0、M8*1.25、M10*1.5、M12*1.75","个/只/台"]
[192,"全封胶枪","15寸","个/只/台"]
[193,"吹气球","大号","个/只/台"]
[194,"橡胶锤","1磅","个/只/台"]
[195,"巡更棒","长约16cm,直径约3cm,防水,LED强光照明,识别3人以上,带闹钟,充电后使用1000次以上,提供10个以上夜光巡更点和管理软件","个/只/台"]
[196,"两用棘开快扳","19mm，全抛光","个/只/台"]
[197,"恒温焊台","工业级智能无铅焊台","个/只/台"]
[198,"油桶搬运车","尺寸1850*880*1280mm，额定载重量300KG","个/只/台"]
[199,"电动疏通机","电机：230V正反转，单相380W,负载钢索转速：165RPM,管内径30-100mm(11/4\"-4\")，最大长度可达30m(100′)","个/只/台"]
[200,"RJ45网络工具（宝工RJ45网络工具）","适用RJ45","个/只/台"]
[201,"划线平台","1000*1000MM，平面精度0.03MM，刮研","个/只/台"]
[202,"充电式液压切刀","适用范围:GJ线≤150mm2，LGJ线≤120mm2，外形尺寸:500*130*40","把"]
[203,"液压切刀","出力:6T，刀口直径:40mm，长度:643mm","个/只/台"]
[204,"充电式液压切刀","切割导线范围:85-150，出力:50KN，切割方式:液压冷切割","个/只/台"]
[205,"单气瓶推车","7301-BK-A;最大承重113.4kg","个/只/台"]
[206,"电锤钻","额定输入功率 1050（W） ，额定电压 220V ","个/只/台"]
[207,"手动液压堆高车","SYC1.0D-30;载重能力1000kg，起升高度3000mm，自重370kg，最低高度90mm，货叉长度900mm","个/只/台"]
[208,"汇流排钻孔工具(含模具）","LS1440，配龙牌电机J1Z-SD04-24A，每套2个磨具","个/只/台"]
[209,"背栓式打孔机","手提便携式背栓打孔机；\n用 途：石材钻孔（背栓孔）；\n适用材料：大理石、花岗岩、陶瓷板材等；\n电压：家用电220v；\n空载转速：9500r/min；\n电流：6.7A；\n机体重量：10KG；\n输入功率：1500W；\n外形尺寸：530*230*305；\n随机配备钻头：M6/M7/M8/M9/M11/M13各10个","个/只/台"]
[210,"型材切割机","220V/50HZ，锯片直径355MM，空载转速3500R/MIN，额定输入功率2000W","个/只/台"]
[211,"混凝土钻孔机","\n类型  金刚石鑽孔机\n空载转速  8400（rpm） \n电源类型  交流电源\n电源电压  220V\n额定输出功率  1450（W）\n电钻结构  直筒式\n钻头夹持方式  空心钻头","个/只/台"]
[212,"ilock联锁专用压线钳","美国泰科电子公司;169481-2;iLOCK联锁机内部压针专用","个/只/台"]
[213,"便携式不锈钢管切管机","管径范围：Φ8-Φ200mm，壁厚0.8-3mm","台"]
[214,"梯车","工作台高2.7米","个/只/台"]
[215,"吸尘器","工业级，5400w","台"]
[216,"真空包装机","适用于精密电子仪器及板卡的真空包装","个/只/台"]
[217,"测试接头","克诺尔;C105707，1","个/只/台"]
[218,"逻辑笔","飞腾三环","个"]
[219,"电缆测试仪（MS2-100）"," 液晶显示：专用 LCD，44.5mm x 21.6 mm 电源：2节 AA 碱性电池 ","个/只/台"]
[220,"电缆故障测试仪","测试范围：1Km/2km/4km/8km，分辨率：1m，测量盲区：0m，手持式，使用环境温度：－15℃－＋45℃","个/只/台"]
[221,"光纤寻障仪","3M;2273M","个/只/台"]
[222,"电缆管道疏通器","12MM","套"]
[223,"手表","防水，可正倒计时，有夜光功能","个/只/台"]
[224,"KOB串口转换器","KT-C10，工业级加强型光电隔离，USB转换器，防雷","套"]
[225,"逻辑笔","LP-200","个/只/台"]
[226,"相序表","输出电压200-480V AC,持续时间限制200V：60 分钟内；480V：4分钟内 ,频率响应20-400Hz ","套"]
[227,"转辙机道岔拉力测试仪（手持式）","双机测试、手持式、3.5吋彩色液晶、支持U盘、支持拍照功能、数据库电脑分析软件、提供手机测试数据远程辅助分析应用程序，可在手机上分析测试数据","块"]
[228,"系统比特误码率及抖动测试仪","CSC-E1DC","个/只/台"]
[229,"蓄电池智能放电测试仪","放电时间:0~99小时59分钟连续可调;最大放电功率:70kw;放电电压:dc 100v~700v;最大放电电流:100a,1—100a放电电流连续可调;电流精度±1%;电流分辨率0.1a;电压精度±0.2%;电压分辨率0.01v","个/只/台"]
[230,"光缆测试仪","贮存温度:-20º C 至 50º C;符合标准:EMI,RFI,EMC;工作温度-10º C 至 50º C;工作湿度95%(10º C~35º C)无冷凝;5%(35º C~40º C)无冷凝;不受控制<10º C;多模光纤验证工具包–包括SimpliFiber Pro光功率计、850/1300多模光源和便携包","套"]
[231,"测量规","科安达;SAHL2","个/只/台"]
[232,"手持式钳口接地电阻测试仪","最大接地电阻1000欧姆（1K 欧姆），最小接地电阻0.010欧姆，分辨率0.001欧姆，电阻测量频率1千赫（1000赫兹），电流测量频率60赫兹，最大电流范围30 A","个/只/台"]
[233,"变频介质损耗测试仪","输入电源：180V-270VAC，50Hz/60Hz±1%，环境温度-10℃到50℃，相对湿度<90%","个/只/台"]
[234,"电话","环境温度：-10~+40℃\n（2）相对温度：10%~95%\n（3）大气压力：86~106kpa\n（4）环境噪音：≤60dB(A)\n（5）振铃声级：≥70dB(A)","个/只/台"]
[235,"弹条扳手","规格尺寸：130×35×12MM，技术参数：Ⅲ型铁路单趾弹条专用工具，功能描述：用于安装弹条扣件","个"]
[236,"转辙机弯嘴钳","用于转辙机内各部件清洁","把"]
[237,"十字镐","镐头38cm，身长约91cm，洋镐","把"]
[238,"铁鞋","铁止轮器，俗称铁鞋，带有卡轨锁，且卡锁可以复位，黄色，连接处牢固可靠，若用螺丝链接，必须使用防松螺母","个/只/台"]
[239,"110kv接地专用杆","有效长度符合国标4.5M，共3根，每根1.5M，快速接头，对接方式不限，但能保证不断","组"]
[240,"双钩紧线器","2T","个/只/台"]
[241,"双钩紧线器","3T","个/只/台"]
[242,"专用卡线器","30AL0822;安全荷载:30KN，3kg，适用线径:∮8-22mm","个/只/台"]
[243,"万能卡线器","20GL0422;安全负荷:20KN(2T)，适用线径:∮4-22mm","个/只/台"]
[244,"起重滑轮组","传动比1:6，含2套吊勾式3轮组，钢丝绳约150m","个/只/台"]
[245,"发黑内六角扳手","17mm，L型，长边长261mm，短边长65mm，尾端倒角方便插入螺帽","个/只/台"]
[246,"尼龙套管钻取设备","轨枕预埋尼龙套管无损取出装置","套"]
[247,"接点压力测试仪","测量范围：0~±150V；显示分辨率：1mV、0.01V、0.1V ；频率测量范围：5～5000Hz ，测量灵敏度要求：不大于10mV/25mA ","个/只/台"]
[248,"液压塞钉拔出器","西安凯信;KXYSB","套"]
[249,"IPC-4300测试仪","4.3寸800*480电容式触摸屏，10/100M自适应，RJ45；内置无线WIFI，速率150M，接收无线网络摄像机图像等2018/8/8 IP摄像机测试 ONVIF（带PTZ云台控制），ACTi、大华IPC-HFW2100P、海康DS-2CD864-E13、三星SNZ-5200、天地伟业TD-NC9200S2、科达IPC120L、霍尼韦尔HICC-2300T、爱谱华顿IP5000-BC-13MP/IRS06-13MP、富尼泰达IPC、富尼泰克kumkang8900、富视捷BY-1080Q、WEISKY IPC等四十多个品牌摄像机。","个/只/台"]
[250,"温枪","-20℃~850℃","个/只/台"]
[251,"函数信号发生器","带宽25 MHz ，250 MS/s ，内存深度128 K，通道2 ","台"]
[252,"光熔接机","单芯熔接机，适用SM (单模), MM (多模), DS (色散位移)光纤, NZDS (非零色散位移，即G.655光纤)；光纤切割长度8-16mm, 被覆光纤直径250µm，16(标准) 或8-16mm (选用)，被覆光纤直径250µm-1000µm；熔接时间：9秒","个/只/台"]
[253,"超声波清洗机","容量：15L ,额定电压：220V ，额定功率：300W ","个/只/台"]
[254,"纸币处理模块大修工具","MEI纸币模块三四级维护专用工具，含安装ω型卡工具Φ1.9、Φ2.3、Φ3.2、Φ4.0、Φ5.0、Φ6.0","套"]
[255,"便携式场强测试仪","工作温度和相对湿度32℉ 至 113℉（0oC 至 +45oC），冲击和振动：随机，2 g，5 Hz — 500 Hz （2级）1 米跌落试验；显示屏：2.8 英寸彩色 LCD（320 x 240 像素）","个/只/台"]
[256,"数字化探伤仪","工作频率 0.5～20MHz \n增益调节 0.0～110.0dB，步进0.1、1.0、2.0、6.0dB，提供智能加速调节功能 \n检测范围 2.0～10000mm（钢纵波），连续可调 \n声速范围 500～15000m/S，连续可调 \n脉冲移位 -20～3000uS \n动态范围 ≥32dB \n垂直线性误差 ≤3% \n水平线性误差 ≤0.1% \n分辨率 ≥36dB \n灵敏度余量 ≥60dB（200mm-ф2mm平底孔） \n电噪声电平 ≤10% \n数据存储 可存1000套探伤报告 \n显示屏 高分辨率（640×480）TFT彩色液晶显示屏6.5\"超大屏幕、高亮度、262144种颜色 \n电源 两种供电方式：\n 大容量锂电池，无记忆效应，连续工作6小时以上\n 220V交流电（配电源适配器） \n环境温度 -30℃～ 60℃ \n","个/只/台"]
[257,"铝合金单桅柱高空作业平台","最大升高高度8米，载重125KG","个/只/台"]
[258,"自动雨伞袋机","铁制340*250*725MM","个/只/台"]
[259,"双卡压连接薄壁不锈钢手持电动工具","艾默生;DN15-DN65","个/只/台"]
[260,"移动音响","移动音响[台湾咪宝;MIPRO MA-202B;无线喊话器，手持高配套装]","个/只/台"]
[261,"手提电动打包机","JD13/16","个/只/台"]
[262,"光纤识别仪","FI-60","个/只/台"]
[263,"视频综合测试仪","MD1802","个/只/台"]
[264,"手持式喊话器配套电池","大大声L-4LA配套电池","节"]
[265,"安检篮","31.5*21.5*17.5cm","个/只/台"]
[266,"轮椅","带手刹，脚踏板可拆缷，防后滑/200*120*68cm","个/只/台"]
[267,"氩气管","外径13MM，壁厚5MM，50M/盘，材料工艺：感性PVC","个/只/台"]
[268,"铜挂锁","长78mm*宽60mm*厚12mm，弯勾直径:7mm，通用钥匙，锁体材质:铜，弯勾材质:钢","个/只/台"]
[269,"紫铜棒","洛铜;Φ30MM*300MM","个/只/台"]
[270,"乙炔软管","30M","盘"]
[271,"圈丝地垫","1.2mx2m、四周压边、厚度：>11.0mm","张"]
[272,"氧气软管","Φ8*2B*30M","盘"]
[273,"不锈钢漏斗","口径140mm，耐酸碱腐蚀","个"]
[274,"钥匙扣","不锈钢双环钥匙扣，匙扣本体6cm，圈内径2.5cm，皮带孔4cm","个/只/台"]
[275,"硬管机油壶","容量250CC，杆长80mm，铝头钢管铝合金阀体","个/只/台"]
[276,"鳄鱼夹","30A，纯铜，每对红黑色各1支","个/只/台"]
[277,"钥匙圈","带铭牌，可任意更换标签纸，50个/盒","盒"]
[278,"消防专用扳手","铸钢，红色防锈涂层，防锈耐用，长300mm","把"]
["    单位名称（加盖公章）："]
["    联系人："]
["    联系方式："]
["备注：提报品牌型号多于2种的，可在“供应商提报描述”中增加相应描述列。如提报物资于需求描述有差异（含包装量差异），请在备注中进行相应说明。\n"]